**Coal lab 12**

Name: Syed Muzzamil Waseem

SID: 11067

Question 1

CODE:

Include Irvine32.inc

.data

.code

divof proc

sub edx,edx

mov ebx,[esp+4]

mov eax,[esp+8]

div ebx

ret 8

divof endp

main proc

mov eax,200

push eax

mov eax,20

push eax

call divof

call writeint

exit

main endp

end main

A computer screen capture

Description automatically generated with medium confidence